To: All Raw Thrills Customers and Distributors			
Date: July 15, 2009
Product: H2Overdrive
Installation Tips: Bill Acceptor, Security, and 36 inch door locations

To Our Valued Customers and Distributors,

Please find important installation tips for installing bill validators, security, and game installation for locations with narrow doorways for H2Overdive, as below.

Bill Acceptor Options
Raw thrills has designed several options to allow operators to use a wide variety of Dollar Bill Acceptors in their H2Overdrive game, depending upon the type of coin door used on the game in manufacturing, and the model dollar bill acceptor the customer prefers. 

These options require some additional items for installation, as outlined below.

H2Overdrive Games built with the Dollar Bill Acceptor Cut-out on the Coin Mechanism Door

Pyramid Option – 12 VDC Up-stacker
DBV model number 5400-UC1-USA 12V
Additional Parts Required:
1 – CA3387 wiring harness

Mars Option – 120 VAC Up-stacker
DBV model number AE-2451-U5E
Additional Parts Required:
1 – CA-3461 wiring harness
1 – CA-3462 wiring harness

Mars Option – 12 VDC Up-Stacker
DBV model number AE2654-U5 
Additional Parts Required:
1 – 810-00124-01 wiring harness

H2Overdrive Games built with the Dollar Bill Acceptor Cut-out on the Cash Door
 
Pyramid Option – 12 VDC Down-Stacker
DBV model number 5400-DC1-USA 12V
Additional Parts Required:
1 – CA-3387 wiring harness
1 – 025X3731-001 Over / Under Cash Box

Mars Option – 120 VAC Down Stacker
DBV model number AE-2431-D5E
Additional Parts Required:
1 – CA3461 wiring harness
1 – CA-3462 wiring harness
1 – 025X3731-001 Over / under Cash Box

Continued on next page
Installation Options for Additional Security

H2Overdrive games built with the Dollar Bill Acceptor Cut-out on the Coin Mechanism Door have 2 options available for additional security, as below.

1 – Part Number 33-9715-00 Bar Hasp (Standard lighter weight Bar across Doors)
Or
1 – Part Number 33-9685-00 Heavy Duty Steel Bar / Plate (heavy Duty / Higher Security)

H2Overdrive games built with the Dollar bill Acceptor cutout on the Cash door have one option available for additional security, as below.

1 – Part Number 33-9780-00 Bar Hasp 

Installation Tips for Locations With Narrow Doors (36” doors)

Please note the H2Overdrive is designed with the ability to be moved through 36” doors, and installed in locations with these types of narrow passageways. The games can be moved through these size doorways by moving the rear cabinet and seat through the door unassembled (Seat not attached to monitor cabinet)

The rear cabinet assembly will fit through most of these size doors by rolling the cabinet through sideways, in most cases without removing the dash / control panel assembly. In some cases, depending upon the depth of the door Jam, it may be necessary to remove the dash / control panel, and than move the game through sideways. 

Thus note, as in Diagram below, in most cases the cabinet width of 34.69 inches will fit through almost all standard 36-inch doors. In rare cases the Dash Board may need to be removed to reduce the cabinet width to 31.78 inches to fit through the 36” doors with deep door jams, as shown diagram below.

Please Contact Betson Imperial Parts and Service at 1-800-828-2048 place an order for any of the optional materials required.

We thank you for your continued support of our products.