To:  All Raw Thrills Customers and Distributors			
Date: May 14, 2007
Product: The Fast and the Furious Drift S/N 1000 to 1540
Re: Monitor Bezel mounting screws

To Our Valued Customers and Distributors,

Raw Thrills engineers have made a change to the screws used to secure the monitor bezel to the cabinet.  The original round head screws may cause unnecessary scratches to the adjacent cabinets side decals when the games are placed side-by-side. The new screw is a flathead type and will not cause these scratches when the cabinets are position side-by-side.  Please refer to the diagram for the position of these screws.

Remove the 4 existing bezel mounting screws using the T27 torx wrench supplied with the game. Replace with the 4 flathead screws and install with the supplied hex wrench.  

If you require any assistance please call 800-753-2513

Thank you

George Angermeyer
Betson Enterprises
303 Paterson Plank Rd.
Carlstadt, N.J. 07072
Phone (800) 524-2343 ext 3331
Fax (201) 438-3372
Gangermeyer@Betson.com